
Please find the following on your diskette:

	CN0170.EXE		A self-extracting ZIP file that holds the following:

	   SOFTWARE MANUAL.PDF	Adobe Acrobat file of the software manual   

	   HARDWARE MANUAL.PDF	Adobe Acrobat file of the hardware manual   

	   USERS GUIDE.PDF	Adobe Acrobat file of the User's Guide   


       	   RUN170.EXE     	A DOS program to operate the CN0170 from a PC. Instructions for the indexer may be
				entered manually from the keyboard or downloaded from an ASCII file.
				Help windows are accessed by pressing <F1>.

      	   RUN170.BAS     	The Basic source file for RUN170.exe

     	              		
       	   SETUP.170     	A sample setup file of parameter instructions for a system with two CN0170s. One axis
				is used on the first CN0170 and both axis are used on the second one. It is not 
				necessary to spell the parameters out, it is done here for clarity and to demonstrate
				the ability to send them this way.

	   READ.ME        	This file!


Copy these files to a directory on your hard drive and run MANUALS.EXE to extract the manuals.

      
Other things ..

1. When daisy-chaining units together jumper pin 13 to pin 19 on the serial connector of the last unit in the chain.
                            
2. If you use the DOS COPY command to download files to the CN0170, the MODE command should include the "p" parameter.

	example:  MODE COM1:1200,n,8,1,p


---------------------------Copyright © 1999 Centent Company, All rights reserved.------------------------------------

